*Příloha č.1 - AIRCRAFT SPECIFICATIONS*

**L-410 UVP “Turbolet”**

**Location:** Pardubice

**s/n:** 810731

**Total Time AF:** 7,479:25 Hours & 13,892 Landings

**Production**: 25.11.1981

**ENGINES:**

GE M-601D: s/n 834046 (outside the aircraft) made in 1983

 total time: 6,035:45

 total of cykles: 7,825

 last GO 2006

GE M-601D: s/n 912008 made in 1991

 total time: 4,498:25

 total of cykles: 6,831

 last GO 2013

**PROPELLER:**

V-508D: s/n 930663304 (outside the aircraft) made in 1999

 total time: 1,325:40

 last GO 2016

V-508D: s/n 110663270 made in 1991

 total time: 4,329:40

 last GO 2011

**AVIONICS:**

CVR: Sigle A 100A

RADAR: Weather RDS-81

RAD ALT: Single KRA 405

COM 1: LUN 3520.15

COM 2: GNS-530W

NAV 1: GNS-530W

NAV 2: KNS-81

XPDR 1: GTX-330D

XPDR 2: KXP-756A

ADF: Dual KDF-806

DME: Dual KDM 706A

GPS: Single GNS-530W (Garmin)

ICS: Dual LUN 3520.91

MARKER: Dual KMR-675

GMK: Dual KCS-55

ELT: ARTEX C 406-2

FDR 39HL

**EXTERIOR:**

Base paint Blue RAL 5012 and RAL 5024, painted last time: 2012

**INTERIOR:**

Number of passengers: Nine (9) or ten (10) according to the number of crew members: three (3) or two (2)

cabin configuration: club seating arrangement with 8 places and two tables and one (two) separated seats

baggage compartment and toilet is at the back of the fuselage

**LAST REVIZION:** date 22.2.2012, hour 5,210:40, TBO Ten (10) years & 4,800 hours

**LAST PERFORMED Inspections:**

6 Mo 19.6.2020

24 Mo 21.1.2020

48 Mo 21.1.2020

300 Hr P2 19.6.2020 by 7,408:20

1,200 Hr P3 27.6.2016 by 6,440:40

